    

Government of Goa

**DIRECTORATE OF SKILL DEVELOPMENT & ENTREPRENEURSHIP**

**BICHOLIM GOVERNMENT INDUSTRIAL TRAINING INSTITUTE**

Valshi, Bicholim – Goa 403504 Phone no.: 0832 - 2362315

Website: [www.itibicholim.goa.gov.in](http://www.itibicholim.goa.gov.in) Email: bicholim-iti.goa@nic.in

No.21/BGITI/STR/Solar Tech./2020-21/834 Date: 30.08.2021

To,

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Sub: - Quotation for Supply of Dead Stock materials for Solar Technician (Electrical of this institute. reg

Sir,

You are requested to kindly furnish your lowest and reasonable rates for the consumable materials as per below mentioned:-

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sr.No** | **Description of item** | **Qty** | **Rate** | **Amount** |
| 1 | **As per Enclosed Annexure-I** |  |  |  |

## Terms and conditions:

1. The materials shall be supplied FOR destination within 15 days of placing supply order at the Bicholim Government Industrial Training Institute, Bicholim Goa.
2. GST and any other levy applicable at the time of supply may be shown **separately** in the quotation; otherwise it will be presumed that the prices offered are inclusive of all taxes.
3. The rate quoted shall be **inclusive** of packing and forwarding charges and freight paid for destination at Bicholim Government Industrial Training Institute, Bicholim Goa.
4. The material will be accepted after the inspection only if the same confirms with the specification mentioned in the supply order.
5. Quotations will be evaluated for all the items together. Therefore, all the items may be quoted.
6. The material if not accepted after inspection shall be collected by the supplier immediately with written assurance to supply the same as per specifications as mentioned in the supply order. The Bicholim Government Industrial Training Institute, Bicholim Goa shall be responsible for security/storing.
7. This office reserves the right to accept or reject any or all the quotations without assigning any reason thereof.
8. The warranty / guarantee shall be furnished as the case may be.
9. The extension of time limit will be granted as per the discretion of the Bicholim Government Industrial Training Institute, Bicholim Goa on genuine grounds by the written request of the supplier.
10. The quotation may be sent in **envelope** superscribing “ QUOTATION NUMBER & SUBJECT” so as to reach this office at 2.30 pm on or before **13/September/2021** which will be opened on the same day at 3.30 pm.

 Yours faithfully,

 ( Kapil p. Aigal )

 Principal

Copy to :- 1) The guard file

 2) O/c

|  |
| --- |
| **ANNEXURE-I** |
| **Sr No** | **Name of the Tool** | **Specification** | **Qty**  | **Units** |
| 1 | Measuring Steel Tape | 5 meter | 21 | Nos |
| 2 | Combination Plier Insulated | 200 mm | 21 | Nos |
| 3 | Screw Driver Insulated | 4 mm X 150 mm, Diamond Head  | 21 | Nos |
| 4 | Screw Driver Insulated | 6 mm X 150 mm | 21 | Nos |
| 5 | Electrician Screw Driver Thin Stem Insulated Handle | 4 mm X 100 mm | 21 | Nos |
| 6 | Heavy Duty Screw Driver Insulated | 5 mm X 200 mm | 21 | Nos |
| 7 | Electrician Screw Driver Thin Stem Insulated Handle | 4 mm X 250 mm | 21 | Nos |
| 8 | Punch Centre | 9 mm X 150 mm | 21 | Nos |
| 9 | Knife Double Bladed Electrician | 100 mm | 21 | Nos |
| 10 | Neon Tester | 500 V | 21 | Nos |
| 11 | Steel Rule Graduated both in Metric and English Unit | 300 mm with precision of 1/4th mm | 21 | Nos |
| 12 | Hammer, cross peen with handle | 200 grams | 21 | Nos |
| 13 | Pipe Vice Cast Iron with Hardened Jaw Open Type | 100 mm | 2 | Nos |
| 14 | File Flat | 200 mm 2nd cut with handle | 2 | Nos |
| 15 | File Half Rround | 200 mm 2nd cut with handle | 2 | Nos |
| 16 | File Round | 200 mm 2nd cut with handle | 2 | Nos |
| 17 | Pliers Long Nose Insulated | 150 mm | 4 | Nos |
| 18 | Gauge, Wire Imperial Stainlees Steel Marked in SWG & mm | Wire Gauge - Metric | 1 | Nos |
| 19 | Pliers Side Cutting | 150 mm | 2 | Nos |
| 20 | Scriber(Knurled Centre Position) |   | 2 | Nos |
| 21 | Pipe Cutter to Cut Pipes | upto 5 cm. dia | 1 | Nos |
| 22 | Pipe Cutter to Cut Pipes | Above 5 cm dia | 1 | Nos |
| 23 | Multi Meter (Analog) | 0 to 1000 M Ohms, 2V to 500 V,100 microA to 10A DC and AC | 1 | Nos |
| 24 | Wire Cutter and Stripper | 150 mm | 4 | Nos |
| 25 | Rooftop Mounting Structure | For 4 x 250 W solar panels mounting practice, with tilt adjustment | 1 | Set |
| 26 | Civil Work Utensils | Spade, Mixing Spoon, Leveling Plates | 1 | Set |
| 27 | Plumbing Tools |   | 1 | Set |
| 28 | Multimeter | Digital 0 to 1000 M Ohms, 2V to 700V,100 microA to 10A DC and AC | 2 | Nos |
| 29 | Solar Insulation Meter Insolation Meter |   | 1 | Nos |
| 30 | Magnetic Flux Meter | 0-500 Tesla | 1 | Nos |
| 31 | Temperature Controlled Soldering Iron | 50 Watt, 230 Volt | 1 | Nos |
| 32 | Solar Cell Based Sunlight Radiation Meter | For Solar power measurement up to 2000 w/square meter | 1 | Nos |
| 33 | Magnetic Compass |   | 4 | Nos |
| 34 | Lead Acid Battery | 12V, 40Ah, 75Ah | 1 | Nos Each |
| 35 | Lead Acid Battery | 12V, 100 Ah | 4 | Nos  |
| 36 | Motorized Bench Grinder | AC Mains Operated | 1 | Nos |
| 37 | Solar Charge Controller with Dusk to Dawn Automatic Switching | 12V, 10A | 4 | Nos |
| 38 | Solar Charge Controller with Manual Switch ( Day Lighting) | 12 V 10 A | 4 | Nos |
| 39 | Array Junction Box | for connecting 250W x 4 Nos. solar panel with DC fuse, DC MCB, and surge suppressor protection | 1 | Nos |
| 40 | Solar Cell Kit |   | 1 | Nos |
| 41 | A.C. Voltmeter M.I | 0 –500V AC | 2 | Nos |
| 42 | Voltmeter | 0 - 30V | 2 | Nos |
| 43 | Voltmeter | 0 - 100V | 2 | Nos |
| 44 | Ammeter MC | 0 - 1A | 2 | Nos |
| 45 | Ammeter MC | 0 - 5A | 2 | Nos |
| 46 | Ammeter MC Centre Zero | 0 - 20A | 2 | Nos |
| 47 | Ammeter MC Centre Zero | 0-50A | 2 | Nos |
| 48 | Power Factor Meter |   | 1 | Nos |
| 49 | Rheostat | 0 -1 Ohm, 5 Amp0 -10 Ohm, 5 Amp0- 25 Ohm, 1 Amp0- 300 Ohm, 1 Amp | 1 | Nos Each |
| 50 | DC Pump | 24V, 0.5HP | 1 | Nos |
| 51 | PWM Controller |   | 1 | Nos |

 ( Kapil p. Aigal )

 Principal